Title=Slovenian
------------------------------------------

1001=Izberi
1002=Znamka
1003=Model/Verzija
1004=Sistem
1005=ECU
1006=Poveži
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Poveži/Auto
1008=Nastavitve
1008T=Change program settings
1009=Novo verzijo programa lahko dobite na
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=Povezujem...
1051=POVEZUJEM Z ECU
1052=Prosim Počakajte
1053=Kontakt mora biti sklenjen.  Pritisnite ESC za prekinitev
1054=Neveljavna ISO koda računalnika
1055=Pritisnite Y za nadaljevnaje oziroma pritisnite N za prekinitev
1056=POVEZAVA NI USPELA
1057=Preverite vaš kabel in nastavitve serijskega vmesnika!
1058=Brez povezave
1059=Pritisnite Y za nadaljevanje
1060=Previsoka zakasnitev!!!
1061=Potrebujete ELM 327/OBDKey vmesnik za povezavo s tem modulom!
1062=Potrebujete VagCom/OBDKey vmesnik za povezavo s tem modulom!
1070=OPOZORILO
1071=Časovna omejitev uporabe zastonjske verzije je omejena na 20 minut. Program se bo zaprl čez eno minuto!
1072=Časovna omejitev uporabe zastonjske verzije je omejena na 20 minut. Program se bo zdaj zaprl!
1073=V zastonjski verziji programa lahko izberete največ 4 parametre hkrati!
1074=Please UNPLUG OBDKey from OBD connector.
1075=Then PLUG OBDKey back and press Y in 10 seconds.
1076=SEND DIAGNOSTIC REPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=The report is ANONYMOUS and does not contain any personal data! Continue? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=Motor
1102=ABS
1103=Airbag
1104=Električni Volan
1105=Menjalnik
1106=Armaturna Plošča
1107=Šasija
1108=Servis
1109=Žarometi
1110=Klimatska naprava
1111=Ostalo
1121=[Recent]

------------------------------------------

2001=Infrmacije
2002=Prekini
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=OPOZORILO: Neveljavna ISO koda za izbrano vozilo!


------------------------------------------

3001=Napake
3002=Pobriši napake
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=Napake niso prisotne
3004=ECU ni zaznal nobene napake
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=BRISANJE SHRANJENIH NAPAK
3051=Lučka prižgana
3052=Prazno
3053=Shranjeno
3054=S prekinitvami
3055=Kritično
3056=Neveljaven signal
3057=Ni signala
3058=Signal nizek
3059=Signal visok
3060=Zaznan trk
3061=S prekinitvami
3062=Prisotno
3065=Vzrok za to napako je neveljaven signal, ki ga je ECU prejel s senzorja.
3066=Vzrok za to napako je da ECU ni prejel signala s senzorja.
3067=Vzrok za to napako je da je ECU prejel zelo nizek signal s senzorja.
3068=Vzrok za to napako je da je ECU prejel zelo visok signal s senzorja.
3070=Vzrok za to napako je
3071=Trenutno stanje napake je
3072=Vrednost števca napak je
3073=Opozorilna lučka na armaturni plošči ni bila aktivirana za to napako.
3074=Opozorilna lučka na armaturni plošči je bila aktivirana za to napako.
3075=Napaka trenutno ni prisotna. Počistite napake in opazujte ali se enaka napaka pojavi čez čas.
3076=Napaka trenutno ni prisotna, ampak je shranjena v spominu. Počistite napake in opazujte ali se enaka napaka pojavi čez čas.
3077=Napaka se pojavlja s prekinitvami. Počistite napake in opazujte ali se enaka napaka pojavi čez čas.
3078=Napaka je prisotna. Naredite ustrezne ukrepe za popravilo napake.
3080=Brez opisa
3081=Ni stika
3082=Kratek stik na maso
3083=Kratek stik na V+ baterije
3084=Ni stika / Kratek stik na maso
3085=Ni stika / Kratek stik na V+ baterije
3086=Vrednost prenizka
3087=Vrednost previsoka
3088=Vrednost konstantna
3089=Verodostojnost
3090=Kratek stik
3091=Zaznana motnja / Neveljaven signal
3092=Slab stik / Ni signala / Airbag sprožen
3093=Neznano / Zategovalniki pasov sproženi
3094=Neznano / Sovoznikov airbag sprožen
3095=Neznano / Notranja napaka
3096=Neznano / Voznikov airbag sprožen
3097=Neznano / Kratek stik
3098=Neznano / Ni napajanja
3099=Neznano

------------------------------------------

4001=Parameteri
4002
4002T=Click this button or press S\rto move selected parameters on top
4003
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Sort. samodejno
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Naloži
4007=Shrani
4008=Dodaj Predlogo
4009=Predloge
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012
4012T=Click this button or press A\rto select all parameters
4013
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Čas

%=%
°C=°C
bar=bar
deg.=deg.
deg./sec.=deg./sec.
G=G
gr/s=gr/s
Kg/h=Kg/h
km=km
km/h=km/h
m/s=m/s
m/sec²=m/sec²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sec
steps=steps
V=V
days=days
l/h=l/h

------------------------------------------

5001=Graf
5002=Min
5003=Max
5004=Datoteka
5004T=CSV files loaded in memory
5005=Start
5005T=Start/stop recording CSV file
5006=Stop
5007=Izvozi
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Uvozi
5008T=Load a previously saved CSV file
5020=Grafi
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Hitrost
5021T=Sampling rate of the parameter values
5022=Skaliranje
5022T=Horizontal scalling factor 
5030=Oznake
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=Aktuatorji
6002=Izvrši
6002T=Execute selected function
6050=PREBERITE VSA NAVODILA
6051=KONČANO
6052=IZVRŠITEV NI USPELA
6053=Nepravilne razmere za izvršbo testa!
6054=Test NI podprt!
6055=Status:
6056=Status: NEZNANO
6057=TURN THE KEY TO OFF
6058=PLEASE CONFIRM
6059=Press ESC to abort
6060=Aborted by user

6061=SECURITY CODE
6062=Invalid security code!
6063=WARNING: The Body Computer blocks for 30 min after 3 attempts!
6064=The Body Computer is blocked
6065=You must wait 30 minutes with key ON to unblock
6066=Security access failed
6067=Undefined error
6068=PREPARE REMOTE CONTROL {0}
6069=Press Y and you will have 15 seconds to press RC button
6070=Press N if you do not have any more remote controls
6071=DETECTING REMOTE CONTROL {0}
6072=Press any RC button for more than 3 seconds
6073=STORING REMOTE CONTROLS

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=AKTIVIRANJE RELEJA KLIME
6201=AKTIVIRANJE PISKAČA
6202=AKTIVIRANJE TULJAVE
6203=AKTIVIRANJE VENTILA EGR
6204=AKTIVIRANJE VENTILA EVAPORACIJE
6205=AKTIVIRANJE MOTORJA PROSTEGA TEKA
6206=AKTIVIRANJE INJEKTORJA
6207=AKTIVIRANJE RELEJA PUMPE GORIVA
6208=AKTIVIRANJE PUMPE
6209=AKTIVIRANJE RELEJA
6210=AKTIVIRANJE ELEKTRO VENTILA
6211=AKTIVIRANJE LUČKE MOTORJA
6212=AKTIVIRANJE EGR VENTILA
6213=AKTIVIRANJE HITREGA PROSTEGA TEKA
6214=AKTIVIRANJE LUČKE GRELNIH SVEČK
6215=AKTIVIRANJE GRELNIH SVEČK
6216=AKTIVIRANJE RELEJA GRELCA
6217=V TEKU
6218=TEST VISOKE HITROSTI VENTILATORJA
6219=TEST NIZKE HITROSTI VENTILATORJA
6220=AKTIVIRANJE AKTUATORJA NASTAVITVE VBRIZGA
6221=PREVERI PREMIK KAZALCA
6222=AKTIVIRANJE OPOZORILNE LUČKE
6223=AKTIVIRANJE OPOZORILNE LUČKE
6224=TEST OPOZORILNE LUČKE
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Prilagoditve
7002=Izvrši
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=Log

8101=Tip vmesnika
8101T=Type of interface
8102=Serijska vrata
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Hitrost
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=Jezik vmesnika
8105=Jezik podatkov
8106=CSV ločilo
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=CSV mapa
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=LOG mapa
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=Predvajaj zvoke
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Barve parametrov
8112=Barva ozadja
8113=Barva mreže
8114=Y-os pisava
8115=X-os pisava
8116=Pisava parametrov
8117=Debelina črte
8118=Spremeni
8119=UI Font (Grids)
8120=UI Font (Buttons)
8121=Show available ports only
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Nastavitve
8192=Splošno
8193=Graf
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Prekliči
8199=OK

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
