Title=Portuguese (PT-PT)
------------------------------------------

1001=Seleccione
1002=Marca
1003=Modelo/Versão
1004=Sistema
1005=ECU
1006=Ligar
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Auto/Ligar
1008=Configurações
1008T=Change program settings
1009=Há uma versão nova do programa em
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=A ligar...
1051=A LIGAR À ECU
1052=Por favor espere...
1053=A ignição deve estar ligada. Prima ESC para cancelar
1054=Código ISO inválido
1055=Prima Y para continuar ou Prima N para cancelar
1056=A LIGAÇÃO FALHOU
1057=Verifique o seu cabo e configurações da porta de série!
1058=DESLIGADO
1059=Prima Y para continuar
1060=Latência muito alta!!!
1061=Precisa de interface ELM 327/OBDKey para ligar a este módulo!
1062=Precisa de interface VagCom/OBDKey para ligar a este módulo!
1070=AVISO
1071=O tempo de limite de cada sessão na versão livre são 20 minutos. O programa vai fechar dentro de 1 minuto!
1072=O tempo de limite de cada sessão na versão livre são 20 minutos. O programa vai agora fechar!
1073=Pode seleccionar até 4 parâmetros na versão LIVRE!
1074=Please UNPLUG OBDKey from OBD connector.
1075=Then PLUG OBDKey back and press Y in 10 seconds.
1076=SEND DIAGNOSTIC REPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=The report is ANONYMOUS and does not contain any personal data! Continue? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=Motor
1102=ABS
1103=Airbag
1104=Direcção Eléctrica
1105=Caixa de Velocidades
1106=Painel de Instrumentos
1107=Carroçaria
1108=Serviço
1109=Faróis
1110=Ar Condicionado
1111=Outro
1121=[Recent]

------------------------------------------

2001=Informações
2002=Desligar
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=AVISO: Código ISO inválido para o sistema de veículo seleccionado!


------------------------------------------

3001=Erros
3002=Apagar Erros
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=Sem erros
3004=Não foram detectados erros pela ECU
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=A APAGAR ERROS
3051=Luz LIGADA
3052=Nenhum
3053=Guardado
3054=Intermitente
3055=Fatal
3056=Sinal Inválido
3057=Sem sinal
3058=Sinal Baixo
3059=Sinal Alto
3060=Ocorrência de Impacto
3061=Intermitente
3062=Presente
3065=A razão para este erro é que a ECU recebeu um sinal inválido do sensor.
3066=A razão para este erro é que a ECU não recebeu um sinal do sensor.
3067=A razão para este erro é que a ECU recebeu um sinal muito baixo do sensor.
3068=A razão para este erro é que a ECU recebeu um sinal muito alto do sensor.
3070=A razão para este erro é
3071=O estado actual deste erro é
3072=O valor do contador de erros é
3073=A luz do painel de instrumentos não foi ligada para este erro.
3074=A luz do painel de instrumentos foi ligada para este erro.
3075=O erro não está a ser detectado. Apague os erros e verifique se o mesmo erro torna a aparecer.
3076=O erro não está a ser detectado, mas está guardado na memória. Apague os erros e verifique se o mesmo erro torna a aparecer.
3077=O erro é intermitente. Apague os erros e verifique se o mesmo erro torna a aparecer.
3078=O erro não está presente neste momento. Tome as medidas adequadas para resolver este erro de sensor.
3080=Genérico
3081=Circuito aberto
3082=Curto-circuito com Massa (GND)
3083=Curto-circuito com +V (Bateria)
3084=Circuito aberto / Curto-circuito com Massa (GND)
3085=Circuito aberto / Curto-circuito com +V (Bateria)
3086=Valor muito baixo
3087=Valor muito alto
3088=Valor constante
3089=Plausibilidade
3090=Curto-circuito
3091=Interferências detectadas / Sinal com falhas
3092=Circuito Aberto / Sem Sinal / Activação do Airbag
3093=Desconhecido / Activação dos Pré-Tensores
3094=Desconhecido / Activação do Airbag do Passageiro
3095=Desconhecido / Erro Interno
3096=Desconhecido / Activação do Airbag do Condutor
3097=Desconhecido / Curto-circuito
3098=Desconhecido / Sem alimentação eléctrica
3099=Desconhecido

------------------------------------------

4001=Parâmetros
4002
4002T=Click this button or press S\rto move selected parameters on top
4003
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Auto Ordenar
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Carregar
4007=Guardar
4008=Adicionar Template
4009=Templates
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012
4012T=Click this button or press A\rto select all parameters
4013
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Tempo

%=%
°C=°C
bar=bar
deg.=deg.
deg./sec.=deg./sec.
G=G
gr/s=gr/s
Kg/h=Kg/h
km=km
km/h=km/h
m/s=m/s
m/sec²=m/sec²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sec
steps=steps
V=V
days=days
l/h=l/h

------------------------------------------

5001=Gráfico
5002=Min.
5003=Max.
5004=Ficheiro
5004T=CSV files loaded in memory
5005=Começar
5005T=Start/stop recording CSV file
5006=Parar
5007=Exportar
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Importar
5008T=Load a previously saved CSV file
5020=Gráficos
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Rácio
5021T=Sampling rate of the parameter values
5022=Escala
5022T=Horizontal scalling factor 
5030=Tags
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=Actuadores
6002=Executar
6002T=Execute selected function
6050=POR FAVOR LEIA TODAS AS NOTAS
6051=COMPLETO
6052=FALHOU A EXECUÇÃO
6053=Condições incorrectas para executar este teste!
6054=Teste NÃO suportado!
6055=Estado:
6056=Estado: DESCONHECIDO
6057=TURN THE KEY TO OFF
6058=POR FAVOR CONFIRME
6059=Press ESC to abort
6060=Aborted by user

6061=SECURITY CODE
6062=Invalid security code!
6063=WARNING: The Body Computer blocks for 30 min after 3 attempts!
6064=The Body Computer is blocked
6065=You must wait 30 minutes with key ON to unblock
6066=Security access failed
6067=Undefined error
6068=PREPARE REMOTE CONTROL {0}
6069=Press Y and you will have 15 seconds to press RC button
6070=Press N if you do not have any more remote controls
6071=DETECTING REMOTE CONTROL {0}
6072=Press any RC button for more than 3 seconds
6073=STORING REMOTE CONTROLS

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=ACTIVAÇÃO DO RELÉ DO SISTEMA DE A/C
6201=ACTIVA A BUZINA
6202=ACTUA A BOBINE
6203=ACTUA A VÁLVULA EGR
6204=ACTUA A VÁLVULA DE PURGA DE VAPORES
6205=ACTUA O ACTUADOR DE RELANTI
6206=ACTUA O INJECTOR
6207=ACTUA O RELÉ DA BOMBA DE COMBUSTÍVEL
6208=ACTUA A BOMBA DE COMBUSTÍVEL
6209=ACTUA O RELÉ
6210=ACTUA A VÁLVULA SOLENÓIDE
6211=LUZ DE AVARIA LIGADA
6212=ACTIVAÇÃO DA VÁLVULA EGR
6213=ACTIVAÇÃO DE RELANTI RÁPIDO
6214=ACTIVAÇÃO DA LUZ DAS VELAS DE INCANDESCÊNCIA
6215=ACTIVAÇÃO DO RELÉ DAS VELAS DE INCANDESCÊNCIA
6216=ACTIVAÇÃO DO RELÉ DE AQUECIMENTO
6217=EM CURSO
6218=LIGA A VENTOÍNHA EM VELOCIDADE RÁPIDA
6219=LIGA A VENTOÍNHA EM VELOCIDADE LENTA
6220=ACTIVAÇÃO DO ACTUADOR DO VARIADOR DE FASE
6221=VERIFICAÇÃO DE MOVIMENTO DAS AGULHAS
6222=ACTIVAÇÃO DA LÂMPADA DE AVISO
6223=ACTIVAÇÃO DA LUZ DE AVISO
6224=TESTE DA LUZ DE AVISO
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Ajustes
7002=Executar
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=REGISTO

8101=Interface
8101T=Type of interface
8102=Porta de Série
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Velocidade
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=Linguagem
8105=Linguagem Dados
8106=Separador do CSV
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=Pasta do CSV
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=Pasta do Registo
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=Tocar Sons
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Côr dos parâmetros
8112=Côr do Fundo
8113=Côr de Grelha
8114=Fonte do Eixo-Y
8115=Fonte do Eixo-X
8116=Fonte dos parâmetros
8117=Espessura da linha
8118=Mudar
8119=UI Font (Grids)
8120=UI Font (Buttons)
8121=Show available ports only
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Definições
8192=Geral
8193=Gráfico
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Cancelar
8199=Aceitar

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
