Title=English
------------------------------------------

1001=Select
1002=Make
1003=Model/Version
1004=System
1005=Control Module
1006=Connect
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Auto/Cn
1008=Settings
1008T=Change program settings
1009=There is a new version of the program at
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=Connecting...
1051=CONNECTING TO ECU
1052=Please Wait
1053=The key must be ON.  Press ESC To Abort
1054=Invalid ISO Code
1055=Press Y To Continue or Press N To Abort
1056=CONNECTION FAILED
1057=Check your cable and serial port settings!
1058=Disconnected
1059=Press Y to continue
1060=Latency Too High!!!
1061=You need ELM 327/OBDKey interface to connect to this module!
1062=You need K-Line/VagCom/OBDKey interface to connect to this module!
1070=WARNING
1071=The running time of free version is limited to 20 minutes. The program will close in 1 minute!
1072=The running time of free version is limited to 20 minutes. The program will now close!
1073=You may select up to 4 parameters in the FREE version!
1074=Please UNPLUG OBDKey from OBD connector.
1075=Then PLUG OBDKey back and press Y in 10 seconds.
1076=SEND DIAGNOSTIC REPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=The report is ANONYMOUS and does not contain any personal data! Continue? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=Engine
1102=ABS
1103=Airbag
1104=Electric Steering
1105=Gearbox
1106=Dashboard
1107=Body
1108=Service
1109=Headlights
1110=Climate control
1111=Other
1121=[Recent]

------------------------------------------

2001=Info
2002=Disconnect
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=WARNING: Invalid ISO code for selected vehicle system!


------------------------------------------

3001=Errors
3002=Clear Errors
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=No fault codes
3004=No fault codes detected by ECU
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=CLEARING STORED FAULT CODES
3051=Light ON
3052=None
3053=Stored
3054=Intermittent
3055=Fatal
3056=Invalid signal
3057=No signal
3058=Signal low
3059=Signal high
3060=Impact occurred
3061=Intermittent
3062=Present
3065=The reason for this fault is that ECU has received invalid signal from the sensor.
3066=The reason for this fault is that ECU did not receive signal from the sensor.
3067=The reason for this fault is that ECU has received very low signal from the sensor.
3068=The reason for this fault is that ECU has received very high signal from the sensor.
3070=The reason for this fault is
3071=The current status of the fault is
3072=The error counter value is
3073=Dashboard warning light was not activated for this fault.
3074=Dashboard warning light was activated for this fault.
3075=The fault is not detected now. Clear fault codes, and observe for future appearance of the same fault.
3076=The fault is not detected now, but it is stored in memory. Clear fault codes, and observe for future appearance of the same fault.
3077=The fault is intermittent. Clear fault codes, and observe for future appearance of the same fault.
3078=The fault is present now. Take appropriate action to fix this sensor fault.
3080=Generic
3081=Open circuit
3082=Short circuit at ground
3083=Short circuit at +V batt
3084=Open circuit / Short circuit at ground
3085=Open circuit / Short circuit at +V batt
3086=Value too low
3087=Value too high
3088=Value constant
3089=Plausibility
3090=Short circuit
3091=Interference detected / Faulty signal
3092=Open circuit / No signal / Airbag impact
3093=Unknown / Pretensioners impact
3094=Unknown / Passenger airbag impact
3095=Unknown / Internal error
3096=Unknown / Driver airbag impact
3097=Unknown / Short circuit
3098=Unknown / No power supply
3099=Unknown

------------------------------------------

4001=Parameters
4002=
4002T=Click this button or press S\rto move selected parameters on top
4003=
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004=
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Auto Up
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Load
4007=Save
4008=Add Template
4009=Templates
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012=
4012T=Click this button or press A\rto select all parameters
4013=
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Time

%=%
°C=°C
bar=bar
deg.=deg.
deg./sec.=deg./sec.
G=G
gr/s=gr/s
Kg/h=Kg/h
km=km
km/h=km/h
m/s=m/s
m/sec²=m/sec²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sec
steps=steps
V=V
days=days
l/h=l/h

------------------------------------------

5001=Graph
5002=Min
5003=Max
5004=File
5004T=CSV files loaded in memory
5005=Start
5005T=Start/stop recording CSV file
5006=Stop
5007=Export
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Import
5008T=Load a previously saved CSV file
5020=Graphs
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Rate
5021T=Sampling rate of the parameter values
5022=Scale
5022T=Horizontal scalling factor 
5030=Tags
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=Actuators
6002=Execute
6002T=Execute selected function
6050=PLEASE READ ALL NOTES
6051=COMPLETED
6052=FAILED TO EXECUTE
6053=Incorrect conditions to run this test!
6054=Test NOT supported!
6055=Status:
6056=Status: UNKNOWN
6057=TURN THE KEY TO OFF
6058=PLEASE CONFIRM
6059=Press ESC to abort
6060=Aborted by user

6061=SECURITY CODE
6062=Invalid security code!
6063=WARNING: The Body Computer blocks for 30 min after 3 attempts!
6064=The Body Computer is blocked
6065=You must wait 30 minutes with key ON to unblock
6066=Security access failed
6067=Undefined error
6068=PREPARE REMOTE CONTROL {0}
6069=Press Y and you will have 15 seconds to press RC button
6070=Press N if you do not have any more remote controls
6071=DETECTING REMOTE CONTROL {0}
6072=Press any RC button for more than 3 seconds
6073=STORING REMOTE CONTROLS

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=A/C SYSTEM RELAY ACTIVATION
6201=ACTIVATES THE BUZZER
6202=ACTUATES THE COIL
6203=ACTUATES EGR VALVE
6204=ACTUATES EVAP. PURGE VALVE
6205=ACTUATES IDLE ACTUATOR
6206=ACTUATES THE INJECTOR
6207=ACTUATES THE FUEL PUMP RELAY
6208=ACTUATES THE PUMP
6209=ACTUATES THE RELAY
6210=ACTUATES THE SOLENOID VALVE
6211=CHECK INDICATOR LIGHT ON
6212=EGR VALVE ACTIVATION
6213=FAST IDLE ACTIVATION
6214=GLOW PLUG LAMP ACTIVATION
6215=GLOW PLUG RELAY ACTIVATION
6216=HEATER RELAY ACTIVATION
6217=IN PROGRESS
6218=RUNS THE FAN AT HIGH SPEED
6219=RUNS THE FAN AT LOW SPEED
6220=TIMING ACTUATOR ACTIVATION
6221=VERIFY NEEDLE SHIFTING
6222=WARNING LAMP ACTIVATION
6223=WARNING LIGHT ACTIVATION
6224=WARNING LIGHT TEST
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Adjustments
7002=Execute
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=Log

8101=Interface Type
8101T=Type of interface
8102=Serial Port
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Speed
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=UI Language
8105=Data Language
8106=CSV Separator
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=CSV Folder
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=LOG Folder
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=Play sounds
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Parameter Colors
8112=Background Color
8113=Grid Color
8114=Y-Axis Font
8115=X-Axis Font
8116=Parameter Font
8117=Line Thickness
8118=Change
8119=UI Font (Grids)
8120=UI Font (Buttons)
8121=Show available COM ports only
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Settings
8192=General
8193=Graph
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Cancel
8199=OK

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
