Title=Nederlands
------------------------------------------

1001=Selecteer
1002=Fabrikant
1003=Model / Versie
1004=Systeem
1005=ECU
1006=Verbinden
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Autom. verb.
1008=Instellingen
1008T=Change program settings
1009=Er is een nieuwe versie van het programma op
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=Verbinden...
1051=Verbonden met ECU
1052=Even wachten A.U.B.
1053=De sleutel moet op "Contact" staan.  ESC om te annuleren
1054=Ongeldige ISO Code
1055=Druk op Y om door te gaan of Druk op N om te stoppen
1056=GEEN VERBINDING TOT STAND GEBRACHT
1057=Controleer je kabel en seriele poort instellingen!
1058=Verbinding verbroken
1059=Druk op Y om door te gaan
1060=Latency Te Hoog!!!
1061=Je hebt een ELM 327/OBDKey interface nodig om te verbinden met deze module!
1062=Je hebt een VagCom/OBDKey interface nodig om te verbinden met deze module!
1070=WAARSCHUWING
1071=The running time of free version is limited to 20 minutes. The program will close in 1 minute!
1072=The running time of free version is limited to 20 minutes. The program will now close!
1073=You may select up to 4 parameters in the FREE version!
1074=Please UNPLUG OBDKey from OBD connector.
1075=Then PLUG OBDKey back and press Y in 10 seconds.
1076=SEND DIAGNOSTIC REPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=The report is ANONYMOUS and does not contain any personal data! Continue? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=Motor
1102=ABS
1103=Airbag
1104=Electric Steering
1105=Versnellingsbak
1106=Dashboard
1107=Body
1108=Service
1109=Koplampen
1110=Climate control
1111=Anders
1121=[Recent]

------------------------------------------

2001=Informatie
2002=Verbinding verbreken
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=WAARSCHUWING: Ongeldige ISO code voor geselecteerd systeem!


------------------------------------------

3001=Fout codes
3002=Verwijder fout code
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=Geen fout codes
3004=Geen fout codes gededecteerd door ECU
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=VERWIJDEREN OPGESLAGEN FOUT CODE'S
3051=Lampen aan
3052=Geen
3053=Opgeslagen
3054=Intermittent
3055=Fataal
3056=Onjuist signaal
3057=Geen Signaal
3058=Signaal laag
3059=Signaal hoog
3060=Impact occurred
3061=Intermittent
3062=Aanwezig
3065=De reden van deze fout is dat de ECU ongeldige signalen heeft ontvangen van de sensor.
3066=De reden van deze fout is dat de ECU geen signalen heeft ontvangen van de sensor
3067=De reden van deze fout is dat de ECU zwakke signalen heeft ontvangen van de sensor.
3068=De reden van deze fout is dat de ECU sterke signalen heeft ontvangen van de sensor.
3070=De reden van deze fout is
3071=De huidige status van de fout is
3072=De fout teller waarde is
3073=Dashboard waarschuwings lampje is niet geactiveerd voor deze fout.
3074=Dashboard waarschuwings lampje is geactiveerd voor deze fout.
3075=De fout wordt nu niet waargenomen, Verwijder de fout codes, en kijk of dezelfde fout zich weer voordoet.
3076=De fout wordt nu niet waargenomen, maar is opgeslagen in het geheugen. Verwijder de fout codes, en kijk of de fout zich weer voordoet.3077=The fault is intermittent. Clear fault codes, and observe for future appearance of the same fault.
3077=The fault is intermittent. Clear fault codes, and observe for future appearance of the same fault.
3078=De fout wordt nu waargenomen. Neem maatregelen om deze sensor te repareren.
3080=Generic
3081=Open circuit
3082=Kortsluiting met Massa
3083=Kortsluiting met +12v van Accu
3084=Open circuit / Kortsluiting met Massa
3085=Open circuit / Kortsluiting met +12v van Accu
3086=Waarde te laag
3087=Waarde te hoog
3088=Waarde constant
3089=Plausibility
3090=Short circuit
3091=Interference detected / Faulty signal
3092=Open circuit / Geen ignaal / Airbag impact
3093=Onbekend / Pretensioners impact
3094=Onbekend / Passenger airbag impact
3095=Onbekend / Interne fout
3096=Onbekend / Bestuurders airbag impact
3097=Onbekend / Kortsluiting
3098=Onbekend / Geen power supply
3099=Onbekend

------------------------------------------

4001=Parameters
4002
4002T=Click this button or press S\rto move selected parameters on top
4003
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Auto Up
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Laden
4007=Opslaan
4008=Add Template
4009=Templates
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012
4012T=Click this button or press A\rto select all parameters
4013
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Tijd

%=%
°C=°C
bar=bar
deg.=deg.
deg./sec.=deg./sec.
G=G
gr/s=gr/s
Kg/h=Kg/h
km=km
km/h=km/h
m/s=m/s
m/sec²=m/sec²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sec
steps=steps
V=V
days=days
l/h=l/h

------------------------------------------

5001=Grafiek
5002=Min
5003=Max
5004=Bestand
5004T=CSV files loaded in memory
5005=Start
5005T=Start/stop recording CSV file
5006=Stop
5007=Exporteer
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Importeer
5008T=Load a previously saved CSV file
5020=Grafieken
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Ratio
5021T=Sampling rate of the parameter values
5022=Schaal
5022T=Horizontal scalling factor 
5030=Tags
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=Actuators
6002=Uitvoeren
6002T=Execute selected function
6050=LEES ALLE NOTITIES A.U.B
6051=UITGEVOERD
6052=NIET UITGEVOERD
6053=Incorrect conditions to run this test!
6054=Test NOT supported!
6055=Status:
6056=Status: Onbekend
6057=TURN THE KEY TO OFF
6058=PLEASE BEVESTIG
6059=Press ESC to abort
6060=Aborted by user

6061=SECURITY CODE
6062=Invalid security code!
6063=WARNING: The Body Computer blocks for 30 min after 3 attempts!
6064=The Body Computer is blocked
6065=You must wait 30 minutes with key ON to unblock
6066=Security access failed
6067=Undefined error
6068=PREPARE REMOTE CONTROL {0}
6069=Press Y and you will have 15 seconds to press RC button
6070=Press N if you do not have any more remote controls
6071=DETECTING REMOTE CONTROL {0}
6072=Press any RC button for more than 3 seconds
6073=STORING REMOTE CONTROLS

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=A/C SYSTEM RELAY ACTIVATION
6201=ACTIVEER DE ZOEMER
6202=ACTIVEER DE BOBINE
6203=ACTIVEER DE EGR KLEP
6204=ACTUATES EVAP. PURGE VALVE
6205=ACTIVEER STATIONAIR KLEP
6206=ACTIVEER BRANDSTOF INJECTEUR
6207=ACTIVEER BRANDSTOFPOMP RELAIS
6208=ACTIVEER POMP
6209=ACTIVEER RELAIS
6210=ACTIVEER THE SOLENOID VALVE
6211=CONTROLEER INDICATIE LICHT aan
6212=EGR KLEP ACTIVEREN
6213=HOOG STATIONAIR ACTIVEREN
6214=GLOEI PLUG LAMP ACTIVEREN
6215=GLOEI PLUG RELAIS ACTIVEREN
6216=VERWARMINGS RELAIS ACTIVEREN
6217=IN VOORBEREIDING
6218=KOEL VENTILATOR OP HOGE SNELHEID
6219=kOEL VENTILATOR OP LAGE SNELHEID
6220=TIMING ACTUATOR ACTIVEREN
6221=VERIFY NEEDLE SHIFTING
6222=WAARSCHUWINGS LAMP ACTIVATION
6223=WARNING LIGHT ACTIVATION
6224=WARNING LIGHT TEST
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Aanpassingen
7002=Uitvoeren
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=Log

8101=Interface Type
8101T=Type of interface
8102=Seriele Poort
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Snelheid
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=UI Taal
8105=Data Taal
8106=CSV Separator
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=CSV Map
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=LOG Map
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=Play sounds
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Parameter Kleuren
8112=Achtergrond Kleuren
8113=Grid Kleur
8114=Y-As Lettertype
8115=X-As Lettertype
8116=Parameter Lettertype
8117=Lijn Dikte
8118=Verander
8119=UI Font (Grids)
8120=UI Font (Buttons)
8121=Show available ports only
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Instellingen
8192=Algemeen
8193=Grafiek
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Annuleer
8199=OK

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
