Title=Magyar
------------------------------------------

1001=Kivalasztas
1002=Tipus
1003=Model/Verzio
1004=Rendszer
1005=ECU
1006=CSATLAKOZAS
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Auto/cn
1008=Beallitas
1008T=Change program settings
1009=uj verzio erheto el
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=Kapcsolodas...
1051=KAPCSOLODAS A VEZERLOHOZ
1052=Kis turelmet
1053=Kapcsolja be a gyujtast.  Megszakitas ESC
1054=Ervenytelen ISO kod
1055=Nyomjon Y A folytatashoz Vagy nyomjon N a megszakitashoz
1056=KAPCSOLODASI HIBA
1057=Ellenorizze a csatlakozasokat es a port beallitast!
1058=Lekapcsolodas
1059=Nyomjon Y a folytatashoz
1060=Idozites tul magas!!!
1061=nem talalhato ELM 327/OBDKey interfesz csatlakoztatva!
1062=Nem talalhato VagCom/OBDKey interfesz csatlakoztatva!
1070=FIGYELMEZTETES
1071=A 20 perces idolimit lejart. A program 1 perc mulva kilep!
1072=Lejart az idolimit. A program most kilep!
1073=4 parameter erejeig valaszthatsz a FREE verzioban!
1074=Please UNPLUG OBDKey from OBD connector.
1075=Then PLUG OBDKey back and press Y in 10 seconds.
1076=SEND DIAGNOSTIC REPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=The report is ANONYMOUS and does not contain any personal data! Continue? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=Motor
1102=ABS
1103=Legzsak
1104=Elektromos kormany
1105=Valto
1106=Muszerfal
1107=Gear
1108=Szerviz
1109=Fenyszorok
1110=Klima
1111=egyeb
1121=[Recent]

------------------------------------------

2001=Informacio
2002=Lekapcsolodas
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=FIGYELEM: ISMERETLEN ISO HIBAKOD A KIVALASZTOTT RENDSZERBEN!


------------------------------------------

3001=Hibak
3002=hibak torlese
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=Nincs hibakod
3004=Nincs tarolt hibakod a kivalasztott vezerloben
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=TORLI A TAROLT HIBAKODOT
3051=MIL BEKAPCSOLT
3052=Nincs
3053=Tarolt
3054=Idoszakos
3055=Vegzetes
3056=Ervenytelen jelzes
3057=NINCS JEL
3058=Alacsony jel
3059=Magas jel
3060=utkozes elofordult
3061=Idoszakos
3062=Jelen
3065=A hiba oka hogy a vezerlo ervenytelen jelzest kapot a szenzortol.
3066=A hiba oka hogy a vezerlo nem kapott jelet a szenzortol.
3067=A hiba oka hogy a vezerlo tul alacsony jelet kapott a szenzortol.
3068=A hiba oka hogy a vezerlo tul magas jelet kapott a szenzortol.
3070=Az ok erre a hibara
3071=A hiba aktualis statusza
3072=The error counter value is
3073=Erre a hibara nem aktivalodott a hibajelzo lampa.
3074=Erre a hibara aktivalodott a hibajelzo lampa.
3075=Hibakodot nem talalt. Torold a meglevo hibakat, A jovoben figyeld aktivalodik e a hiba ujra.
3076=A hiba most nem talalhato,valoszinuleg eltarolodott a memoriaban. torold a hibakodokat es ismeteld meg a kiolvasast
3077=A hiba idoszakos.
3078=A hiba jelen van!itt a lehetoseg hogy torolje.
3080=Generic
3081=Nyitott aramkor
3082=Rovidzarlat -v batt
3083=Rovidzarlat +V batt
3084=Nyitott aramkor / Nem talalhato -v batt
3085=Nyitott aramkor / Aramkor szakadt nem talalhato +V batt
3086=Tul alacsony ertek
3087=Tul magas ertek
3088=Allando ertek
3089=Elfogadhato
3090=Rovidzarlat
3091=Beavatkozast erzekelt / Hibas jelzes
3092=Nyitott aramkor / Nincs jel / Legzsak hiba
3093=Unknown / Ovfeszito hiba
3094=Unknown / Utasoldali legzsak hiba
3095=Unknown / Belso hiba
3096=Unknown / Vezetooldali legzsak hiba
3097=Unknown / rovidzarlat
3098=Unknown / Nincs aramellatas
3099=Unknown

------------------------------------------

4001=Parameterek
4002
4002T=Click this button or press S\rto move selected parameters on top
4003
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Auto Up
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Betolt
4007=Mentes
4008=Uj sablon hozzadasa
4009=Sablon
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012
4012T=Click this button or press A\rto select all parameters
4013
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Ido

%=%
°C=°C
bar=bar
deg.=deg.
deg./sec.=deg./sec.
G=G
gr/s=gr/s
Kg/h=Kg/h
km=km
km/h=km/h
m/s=m/s
m/sec²=m/sec²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sec
steps=steps
V=V
days=nap
l/h=l/h

------------------------------------------

5001=Grafikon
5002=Minimum
5003=Maximum
5004=Fбjl
5004T=CSV files loaded in memory
5005=Inditas
5005T=Start/stop recording CSV file
5006=Leallitas
5007=Export
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Import
5008T=Load a previously saved CSV file
5020=Grafikon
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Arany
5021T=Sampling rate of the parameter values
5022=Mertekegyseg
5022T=Horizontal scalling factor 
5030=Cimke
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=Actuators
6002=Execute
6002T=Execute selected function
6050=KERLEK OLVASD EL AZ OSSZES FELJEGYZEST
6051=KESZ
6052=HIBA A VEGREHAJTASBAN
6053=Nem megfelelo feltetelek a teszt futtatasahoz!
6054=Teszt NEM tбmogatott!
6055=Statusz:
6056=Statusz: ISMERETLEN
6057=TURN THE KEY TO OFF
6058=KÉRJÜK, ERŐSÍTSE MEG
6059=Press ESC to abort
6060=Aborted by user

6061=SECURITY CODE
6062=Invalid security code!
6063=WARNING: The Body Computer blocks for 30 min after 3 attempts!
6064=The Body Computer is blocked
6065=You must wait 30 minutes with key ON to unblock
6066=Security access failed
6067=Undefined error
6068=PREPARE REMOTE CONTROL {0}
6069=Press Y and you will have 15 seconds to press RC button
6070=Press N if you do not have any more remote controls
6071=DETECTING REMOTE CONTROL {0}
6072=Press any RC button for more than 3 seconds
6073=STORING REMOTE CONTROLS

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=A/C RELE AKTIVБLБS
6201=AKTIVALJA A BUZZER-T
6202=AKTIVALJA A TEKERCSET
6203=AKTIVALJA AZ EGR SZELEPET
6204=AKTIVALJA AZ EVAP SZELEPET
6205=ACTUATES IDLE ACTUATOR
6206=AKTIVALJA AZ INJECTORT
6207=AKTIVALJA AZ UZEMANYAG SZIVATTYU RELE-T
6208=AKTIVALJA AZ UZEMANYAG SZIVATTYUT
6209=AKTIVALJA A RELE-T
6210=AKTIVALJA A SOLENOID SZELEPET
6211=ELLENORZO LAMPA BEKAPCSOLAS
6212=EGR SZELEP AKTIVALAS
6213=FAST IDLE ACTIVATION
6214=IZZITAS LAMPA AKTIVALAS
6215=IZZITORELE AKTIVALAS
6216=FUTOTEST RELE AKTIVALAS
6217=FOLYAMATBAN
6218=MUKЦDTETNI A VENTILATORT NAGY SEBESSEGEN
6219=MUKЦDTETNI A VENTILATORT ALACSONY SEBESSEGEN
6220=TIMING ACTUATOR ACTIVATION
6221=VALTS AT MEGFELELO DIAGNOSZTIKAI SZALRA
6222=FIGYELMEZTETO LAMPA AKTIVALAS
6223=JELZOLAMPA AKTIVALAS
6224=MILL LAMPA TESZT
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Korrekcio
7002=Vegrehajt
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=Log

8101=Interfesz tipusa
8101T=Type of interface
8102=Port beallitas
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Sebesseg
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=Program Nyelv
8105=Adat nyelv
8106=CSV elvalasztas
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=CSV Mappa
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=LOG Mappa
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=Hang bekapcsolas
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Parameter szinei
8112=Hatter szine
8113=kijeloles szine
8114=Y-Axis Betutipus
8115=X-Axis Betutipus
8116=betutipus
8117=Vonal suruseg
8118=Valtoztat
8119=UI Font (Grids)
8120=UI Font (Buttons)
8121=Show available ports only
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Beallitas
8192=fo beallitasok
8193=Megjelenites
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Megsem
8199=OK

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
