Title=Español
------------------------------------------

1001=SELECCIONAR
1002=MARCA
1003=MODELO
1004=GESTIÓN
1005=ECU
1006=Conectar
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Auto / Cn
1008=Opciones
1008T=Change program settings
1009=Esta es la nueva versión del Programa
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=CONECTANDO...
1051=CONECTANDO CON LA ECU
1052=Por favor espera...
1053=La llave esta puesta en "ON" (Contacto dado).  Presiona "ESC" Para cancelar
1054=Codigo "ISO" no valido
1055=Presiona "Y" Para continuar o Presiona "N" Para cancelar
1056=CONEXIÓN  FALLIDA
1057=Revisa tu cable y las opciones del puerto en serie!!!
1058=Desconectado
1059=Presiona "Y" para continuar
1060=Latencia muy Alta!!!
1061=Necesitas una interface ELM 327/OBDKey para conectarte a este modulo!
1062=Necesitas una interface VagCom/OBDKey para conectarte a este modulo!
1070=ADVERTENCIA!!!
1071=EL TIEMPO DE FUNCIONAMIENTO DE LA VERSIÓN GRATIS ES LIMITADO A 20 MINUTOS. EL PROGRAMA PODRIA CERRARSE EN 1 MINUTO!!!!
1072=EL TIEMPO DE FUNCIONAMIENTO DE LA VERSIÓN GRATIS ES LIMITADO A 20 MINUTOS. EL PROGRAMA SE VA A CERRAR!!!!
1073=Solo puedes seleccionar 4 parametros en la versión gratis!
1074=Please UNPLUG OBDKey from OBD connector.
1075=Then PLUG OBDKey back and press Y in 10 seconds.
1076=SEND DIAGNOSTIC REPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=The report is ANONYMOUS and does not contain any personal data! Continue? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=MOTOR
1102=ABS
1103=AIRBAG
1104=DIRECCIÓN ELECTRÓNICA
1105=CAJA DE CAMBIOS
1106=CUADRO DE MANDOS
1107=CHASIS (Body)
1108=SERVICIO
1109=LUCES
1110=CONTROL DEL CLIMA
1111=OTROS
1121=[Recent]

------------------------------------------

2001=Información
2002=DESCONECTADO
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=AVISO: Codigo "ISO" no valido para el sistema del vehiculo seleccionado!!


------------------------------------------

3001=Errores
3002=Borrar errores
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=No hay códigos de avería
3004=No hay códigos de avería detectados por la ECU 
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=BORRAR LOS CÓDIGOS DE AVERÍA MEMORIZADOS EN LA ECU
3051=Luz encendida
3052=Nada
3053=Guardado
3054=Intermitente
3055=Fatal
3056=SEÑAL NO VALIDA!!!
3057=SIN SEÑAL
3058=SEÑAL BAJA
3059=SEÑAL ALTA
3060=Impacto producido
3061=Intermitente
3062=Presente
3065=La razón de esto es culpa de que la ECU ha recibido señal no válida del sensor.
3066=La razón de esto es culpa de que la ECU no ha recibido la señal del sensor. 
3067=La razón de esto es culpa de que la ECU ha recibido señal muy baja del sensor. 
3068=La razón de esto es culpa de que la ECU ha recibido señal muy alta del sensor.
3070=La razón de este fallo es
3071=El estado actual del fallo es
3072=El valor del contador de errores es
3073=La luz del salpicadero de alerta no se activó por esta fallo.
3074=La luz del salpicadero de alerta fue activada por esta fallo.
3075=El fallo no ha sido detectado ahora. Borrar los códigos de avería, y observa si en el futuro aparece el mismo fallo. 
3076=El fallo no ha sido detectado ahora , Pero esta memorizado en la memoria. Borra los codigos de averia, y observa si en el futuro aparece el mismo fallo.
3077=El fallo es intermitente. Borra los códigos de avería, y observa si vuelve a aparecer el mismo fallo. 
3078=El fallo está presente. Toma las medidas necesarias para corregir esta fallo del sensor. 
3080=Generico
3081=Circuito abierto
3082=Cortocircuito en masa
3083=Cortocircuito +V en batt 
3084=Circuito abierto / Cortocircuito a masa 
3085=Circuito abierto / Cortocircuito +V en batt 
3086=El valor es demasiado Bajo
3087=El valor es demasiado Alto
3088=Valor constante
3089=Plausibilidad 
3090=Cortocircuito
3091=Interferencias detectadas / Señal defectuosa 
3092=Circuito abierto / No hay señal / Airbag de impacto 
3093=Desconocido / Pretensores de impacto 
3094=Desconocido / Airbag de impacto del pasajero
3095=Desconocido / Error interno
3096=Desconocido / Airbag de impacto del conductor 
3097=Desconocido / Cortocircuito 
3098=Desconocido / No hay fuente de alimentación 
3099=Desconocido

------------------------------------------

4001=Parámetros
4002
4002T=Click this button or press S\rto move selected parameters on top
4003
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Arriba automatico
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Cargar
4007=Guardar
4008=Añadir Plantilla
4009=Plantillas
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012
4012T=Click this button or press A\rto select all parameters
4013
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Tiempo

%=%
°C=°C
bar=bar
deg.=deg.
deg./sec.=deg./sec.
G=G
gr/s=gr/s
Kg/h=Kg/h
km=km
km/h=km/h
m/s=m/s
m/sec²=m/sec²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sec
steps=steps
V=V
days=days
l/h=l/h

------------------------------------------

5001=Grafico
5002=Minimo
5003=Máximo
5004=Fichero
5004T=CSV files loaded in memory
5005=EMPEZAR
5005T=Start/stop recording CSV file
5006=PARAR
5007=Exportar
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Importar
5008T=Load a previously saved CSV file
5020=Graficos
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Tasa
5021T=Sampling rate of the parameter values
5022=Escala
5022T=Horizontal scalling factor 
5030=Preguntas
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=ACTUADOR
6002=EJECUTAR
6002T=Execute selected function
6050=POR FAVOR REVISA TODAS LAS NOTAS
6051=COMPLETADO
6052=FALLO AL EJECUTAR
6053=Condiciones incorrectas para empezar esta prueba!
6054=Prueba "NO" soportada!!!
6055=Estado:
6056=Estado: DESCONOCIDO
6057=TURN THE KEY TO OFF
6058=PLEASE CONFIRM
6059=Press ESC to abort
6060=Aborted by user

6061=SECURITY CODE
6062=Invalid security code!
6063=WARNING: The Body Computer blocks for 30 min after 3 attempts!
6064=The Body Computer is blocked
6065=You must wait 30 minutes with key ON to unblock
6066=Security access failed
6067=Undefined error
6068=PREPARE REMOTE CONTROL {0}
6069=Press Y and you will have 15 seconds to press RC button
6070=Press N if you do not have any more remote controls
6071=DETECTING REMOTE CONTROL {0}
6072=Press any RC button for more than 3 seconds
6073=STORING REMOTE CONTROLS

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=ACTIVACIÓN DE RELE SISTEMA A/C  
6201=ACTIVAR EL ZUMBADOR
6202=ACTUADOR DE LA BOBINA
6203=ACTUADOR VÁLVULA EGR
6204=ACTUADOR VÁLVULA DE PURGA SISTEMA EVAP.
6205=ACTUADOR SENSOR MARIPOSA
6206=ACTUADOR DEL INYECTOR
6207=ACTUADOR DEL RELE DE LA BOMBA DE COMBUSTIBLE.
6208=ACTUADOR DE LA BOMBA
6209=ACTUADOR DEL RELE
6210=ACTUADOR DE LA VÁLVULA SOLENOIDE
6211=REVISIÓN LUZ INDICADORA DE ENCENDIDO
6212=ACTIVACIÓN VÁLVULA EGR
6213=ACTIVACIÓN RAPIDA DE MARIPOSA
6214=LAMPARA ACTIVACIÓN BUJÍA
6215=ACTIVADOR RELE DE DE BUJÍA
6216=ACTIVADOR RELE CALENTADOR
6217=EN PROCESO
6218=PONER EL VENTILADOR A LA VELOCIDAD MAS ALTA
6219=PONER EL VENTILADOR A LA VELOCIDAD MAS BAJA
6220=ACTUATOR ACTIVADOR DE TIEMPO
6221=VERIFICAR AGUJA DEL CAMBIO
6222=ACTIVACIÓN DE LUZ DE AVISO
6223=ACTIVACIÓN DE LUZ DE ADVERTENCIA
6224=PRUEBA DE LUZ DE ADVERTENCIA
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Ajustes
7002=EJECUTAR
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=Registro

8101=Tipo de interface
8101T=Type of interface
8102=Puerto Serial
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Velocidad
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=Lenguaje UI
8105=Lenguaje Codigos
8106=Separador "CSV"
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=Carpeta del "CSV"
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=Carpeta del "LOG"
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=Sonidos
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Colores de los parametros
8112=Color de Fondo
8113=Color de cuadrícula
8114=Fuente Eje-Y
8115=Fuente Eje-X 
8116=Fuente de los Parámetros
8117=Grosor de línea
8118=Cambiar
8119=UI Font (Grids)
8120=UI Font (Buttons)
8121=Show available ports only
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Opciones
8192=General
8193=Grafico
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Cancelar
8199=Confirmar

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
