Title=Danish
------------------------------------------

1001=Vælg
1002=Mærke
1003=Model/Version
1004=System
1005=ECU
1006=Tilslut
1006T=Connect to selected module.\rYou can press CTRL-F10 to connect in 'simulation' mode.
1007=Auto/Scan
1008=Indstillinger
1008T=Change program settings
1009=Der er en ny program version tilgængelig på
1010=Scan
1010T=Scan your vehicle for available modules
1011=Send Report
1011T=Send a diagnostic report to MULTIECUSCAN server.\rThe report contains information about your last connection.
1012=Model
1013=Version
1016=Simulate
1017=Scan DTC
1017T=Scan your vehicle for available modules and check each module for errors

1041=CONNECT ADAPTER 1/GREEN (OR PIN {0})
1042=CONNECT ADAPTER 2/RED (OR PIN {0})
1043=CONNECT ADAPTER 3/YELLOW
1044=CONNECT 3-PIN ADAPTER
1045=If your vehicle has a 3-pin connector then connect a 3-pin adapter only!
1050=Tilslutter...
1051=TILSLUTTER TIL ECU
1052=Vent Venligst
1053=Tændingsnøglen skal sættes til  position on.  Tryk ESC for at afbryde
1054=Forkert ISO Kode
1055=Tryk Y for at fortsætte eller Tryk N for at afbryde
1056=DET VAR IKKE MULIGT AT TILSLUTTE
1057=Undersøg dit kabel og indstillingerne for den virtuelle COMPORT i enhedshåndtering!
1058=Frakoblet
1059=Tryk Y for at fortsætte
1060=Latency for høj,SKAL ændres i Kontrolpanel!!!
1061=Du skal benytte ElmScan 327/OBDKey for at tilslutte til dette modul!
1062=Du skal benytte KKL/OBDKey kabel for at tilslutte til dette modul !
1070=ADVARSEL
1071=Gratis versionen er begrænset til max 20min. Programmet lukker om 1 minut 
1072=Gratis versionen er begrænset til max 20min. Programmet lukker nu ! 
1073=Du kan højest vælge 4 parametre i GRATIS versionen. 
1074=Fjern venligst OBDKey stikket fra konnectoren .
1075=Sæt OBDKey stikket i igen og tryk på Y i 10 sekunder.
1076=SEND DIAGNOSE RAPPORT
1077=Diagnostic report of your last session will be sent to MULTIECUSCAN server.
1078=Rapporten er anonym og indeholder ingen personlige oplysninger! Fortsætte? Press Y or N
1079=SENDING DIAGNOSTIC REPORT
1080=SENDING FAILED
1081=Too many new modules detected!
1082=Too many removed modules detected!
1083=This vehicle is properly configured. PROXI Alignment is not needed!
1084=Reading CAN configuration data ...
1085=Unreliable communication detected!
1086=CURRENTLY CONFIGURED CAN MODULES:
1087=CURRENTLY AVAILABLE CAN MODULES:
1088=NEW CAN MODULES:
1089=REMOVED CAN MODULES:
1090=CAN MODULES THAT REQUIRE EOL PROGRAMMING:
1091=Writing to module:
1092=SUCCESS
1093=FAILED
1094=Writing CAN configuration data ...
1095=Suitable interface not found!
1096=Testing for interface on {0} ...
1097=VagCom/KKL interface found at port {0}
1098={0} interface found at port {1}, speed {2}bps
1099=Scanning ...
1200=WARNING: This interface is not compatible with ELM 327 1.3! Will not connect to any CAN module.
1201=This interface is compatible with ELM 327 1.3! Should connect properly with all CAN modules.
1202=This interface is compatible with ELM 327 1.4! Should connect properly with all CAN modules.
1203=THE ODOMETER VALUE CAN ONLY BE INCREASED!

1101=Motor
1102=ABS
1103=Airbag
1104=Servostyring
1105=Gearkasse
1106=Speedometer
1107=Body
1108=Service
1109=Forlys
1110=Klimaanlæg
1111=Andet
1121=[Recent]

------------------------------------------

2001=Info
2002=Afbryd
2002T=Disconnect from vehicle.\rYou can also press F11 to disconnect
2003=ADVARSEL: Forkert ISO kode for valgte køretøjs system!


------------------------------------------

3001=Fejl
3002=Slet Fejl
3002T=Clear error codes in ECU.\rNOTE: Some errors may not clear if the problem is not fixed.\rYou can also press F10 to clear the errors
3003=Ingen fejl koder
3004=Ingen fejl koder detekteret af ECU
3047=ERROR DETAILS:
3048=Reading error codes...
3049=READING ERROR CODES:
3050=SLETTER GEMTE FEJL KODER
3051=Lys TÆNDT
3052=Ingen
3053=Gemte
3054=Periodisk
3055=Fatal
3056=Forkert signal
3057=Ingen signal
3058=Signal lavt
3059=Signal højt
3060=Impact opstået
3061=Periodisk
3062=Tilstede
3065=Grunden til denne fejl er, at ECU'en har modtaget forkert signal fra sensoren.
3066=Grunden til denne fejl er, at ECU'en ikke har modtaget signal fra sensoren.
3067=Grunden til denne fejl er, at ECU'en har modtaget meget lavt signal fra sensoren.
3068=Grunden til denne fejl er, at ECU'en har modtaget meget højt signal fra sensoren.
3070=Grunden til denne fejl er
3071=Den nuværende status for denne fejl er
3072=Fejl tæller værdien er
3073=MIL lampen blev ikke aktiveret pga. denne fejl.
3074=MIL lampen blev aktiveret pga. denne fejl.
3075=Fejlen er ikke tilstede nu.  Slet fejl koder, og se om fejlen opstår igen
3076=Fejlen er ikke tilstede nu, men den er gemt i hukommelsen. Slet fejl koder, og se om fejlen opstår igen.
3077=Fejlen er periodisk. Slet fejl koder, og se om fejlen opstår igen.
3078=Fejlen er tilstede nu. Foretag det nødvendige, for at reparere denne sensor.
3080=Generisk
3081=kredsløb åbent
3082=Kredsløb kortsluttet til stel
3083=Kredsløb kortsluttet Til Batteri +
3084=kredsløb åbent / Kredsløb kortsluttet til stel
3085=kredsløb åbent / Kredsløb kortsluttet Til Batteri +
3086=Værdi for lav
3087=Værdi for høj
3088=Værdi konstant
3089=Sansynlighed
3090=Kredsløb kortsluttet
3091=Støjsignal fundet / fejlbehæftet signal
3092=kredsløb åbent / ingen signal / Airbag impact
3093=Unknown / Selestrammere impact
3094=Unknown / Passenger airbag impact
3095=Unknown / Intern fejl
3096=Unknown / fører airbag impact
3097=Unknown / Kredsløb kortsluttet
3098=Unknown / ingen strømforsyning
3099=Unknown

------------------------------------------

4001=Parametre - Live data
4002
4002T=Click this button or press S\rto move selected parameters on top
4003
4003T=Click this button or press L\rto sort parameters alphabetically by name
4004
4004T=Click this button or press U\rto sort parameters alphabetically by units
4005=Auto til top
4005T=Turn ON or OFF automatic moving of selected parameters on top
4006=Hent
4007=Gem
4008=Tilføj Skabelon
4009=Skabeloner
4009T=Manage templates
4010=Monitor DTCs
4010T=Turn ON or OFF error code monitoring.\rThis function will continuously check the ECU for errors\rand show a message when new errors appear.\rWhen this function is ON the error codes will be recorded\rinto the CSV files as well.
4011=The following DTCs are present:
4012
4012T=Click this button or press A\rto select all parameters
4013
4013T=Click this button or press N\rto unselect all parameters
4050=READING PARAMETERS:
4101=Tid

%=%
°C=°C
bar=bar
deg.=grader.
deg./sec.=grader./sek.
G=G
gr/s=gr/s
Kg/h=Kg/t
km=km
km/h=km/t
m/s=m/s
m/sec²=m/sek²
mA=mA
A=A
mBar=mBar
mg/i=mg/i
Min=Min
mm=mm
mm³/i=mm³/i
ms=ms
mV=mV
Nm=Nm
rpm=rpm
sec=sek
steps=skridt
V=V
days=dage
l/h=l/h

------------------------------------------

5001=Graf
5002=Min
5003=Max
5004=File
5004T=CSV files loaded in memory
5005=Start
5005T=Start/stop recording CSV file
5006=Stop
5007=Export
5007T=Save the selected CSV file.\rNOTE: All CSV files are automatically saved in your 'CSV Folder'
5008=Import
5008T=Load a previously saved CSV file
5020=Grafer
5020T=Number of graphs to be displayed on the screen.\rYou can select the parameters to be includes in each of the graphs\rby the checkboxes in the left pane.
5021=Rate
5021T=Sampling rate of the parameter values
5022=Scale
5022T=Horizontal scalling factor 
5030=Tags
5041=Time (Δt)
5041T=Select which parameter will be used for the x-Axis.\rIf you select 'Δt' then the parameter data will be drawn as a function of time (i.e. you will see how parameter changes over time).\rIf you select a parameter (Engine speed for example) then the change of other parameters will be drawn as a function of Engine speed.

------------------------------------------

6001=Aktuatorer
6002=Udfør
6002T=Execute selected function
6050=LÆS VENLIGST ALLE NOTER
6051=UDFøRT
6052=UDFØRSEL FEJLET
6053=Forhold ikke korrekte for udførsel af denne test!
6054=Test IKKE understøttet!
6055=Status:
6056=Status: UKENDT
6057=TURN THE KEY TO OFF
6058=BEKRÆFT VENLIGST
6059=Press ESC to abort
6060=Aborted by user

6061=SIKKERHEDS KODE
6062=Forkert sikkerheds kode!
6063=ADVARSEL: Body Computer blokerer i 30 min efter 3 forsøg!
6064=Body Computer er blokeret
6065=Du må vente 30 minutter med tænding på ON for at oplåse modulet
6066=sikkerheds adgang fejl
6067=ukendt fejl
6068=KLARGøR FJERNBETJENING {0}
6069=Tryk Y herefter har du 15 sekunder til at trykke RC knappen
6070=Tryk N hvis du ikke ønsker flere fjernbetjeninger
6071=DETEKTERER FJERNBETJENING {0}
6072=Tryk vilkårlig RC knap i mere en 3 sekunder
6073=GEMMER FJERNBETJENINGER

6081=Aborting...
6082=ABORTED

6101=EXECUTING ACTUATOR...

6200=A/C SYSTEM RELÆ AKTIVERING
6201=AKTIVERER SUMMER
6202=AKTIVERER SPOLEN
6203=AKTIVERER EGR VENTIL
6204=AKTIVERER EVAP. FORDAMPNINGS VENTIL
6205=AKTIVERER TOMGANGS AKTUATOR
6206=AKTIVERER INDSPRØJTNINGS DYSE
6207=AKTIVERER BRÆNDSTOF PUMPERELÆ
6208=AKTIVERER PUMPEN
6209=AKTIVERER RELÆET
6210=AKTIVERER SOLENOIDEVENTIL
6211=CHECK INDICATOR LYS ON
6212=EGR VENTIL AKTIVERING
6213=HURTIG TOMGANGS AKTIVERING
6214=GLØDE RØRS LAMPE AKTIVERING
6215=GLØDE RØRS RELÆ AKTIVERING
6216=VARMERELÆ AKTIVERING
6217=ARBEJDER
6218=KØRER VENTILATOR PÅ HØJ HASTIGHED
6219=KØRER VENTILATOR PÅ LAV HASTIGHED
6220=TIMINGS AKTUATOR AKTIVERING
6221=VERIFICERE NÅLE SKIFTNING
6222=ADVARSELSLAMPE AKTIVERING
6223=ADVARSELSLYS AKTIVERING
6224=ADVARSELSLYS TEST
6225=WRITING PROXI DATA

6501=Unknown error
6502=Timeout error
6503=Generic error
6504=Unsupported function error
6505=Busy error
6506=Incorrect conditions error
6507=Request out of range error
6508=Data out of range error
6509=Configuration not supported by system error

------------------------------------------

7001=Justeringer
7002=Udfør
7002T=Execute selected function
7101=EXECUTING ADJUSTMENT...
7102=Old value
7103=New value

------------------------------------------

8001=Log

8101=Interface Type
8101T=Type of interface
8102=Seriel Port
8102T=The serial port where your interface is connected.\rPLEASE NOTE: The USB interfaces do have serial port numbers as well!
8103=Hastighed
8103T=Serial port speed.\rMost ELM interfaces use 38400, but some use 9600.\rThe OBDKey interface uses 9600.
8104=Bruger Sprog
8105=Data Sprog
8106=CSV Separator
8106T=Separator character for the generated CSV files.\rIt is usually comma, but some countries use comma as decimal separator.
8107=CSV Folder
8107T=A folder where to automatically save\rthe generated CSV files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_CSV
8108=LOG Folder
8108T=A folder where to automatically save\rthe generated LOG files.\rThe folder must exist!\rExample:\rC:\MULTIECUSCAN_LOGS
8109=afspil lyde
8110=IP Address
8110T=The IP Address and port of the WiFi interface.\rFor example: 192.168.0.10:35000 
8111=Parameter Farver
8112=Baggrunds Farver
8113=Grid Farver
8114=Y-Axe Font
8115=X-Axe Font
8116=Parameter Font
8117=Linie Tykkelse
8118=Ændre
8119=UI Font (Linier)
8120=UI Font (Knapper)
8121=Vis kun tilgængelige porte
8121T=Automatically detect which COM ports\rare available on this computer\rand list only those ports.
8122=KWP2000 Timings
8122T=Connection optimizations for KWP2000 protocol used when connecting to most of the engines using VagCom/KKL interface.\rYou can select 'DEFAULT' for no optimizations.\r'FAST' and 'OPTIMAL' will give the best parameter reading rate, but may not work for all vehicles.\r'SLOW' should give more stable connection on slow computers.
8123=Interface 1
8124=Interface 2
8125=Interface 3
8126=Interface 4
8127=Scan For Interfaces
8127T=This function will scan for interfaces connected to your computer.\rThe interfaces must be connected to a car as well.
8128=User Interface
8129=Export && Logging
8130=Show "Please connect Adapter..." message before connecting
8131=Convert kilometers to miles
8132=Redraw frequency
8132T=This controls the repaint frequency of parameters and graph data.\rSelect 'Fast' for for smoother real-time graph.\rSelect 'Slow' if you have disconnection problems when viewing parameters or recording a graph.
8133=High latency mode
8133T=Use this option ONLY for computers with high latency problems.\rIt is recommended to use this option when the VagCom/KKL interface test reports >10ms latency.
8134=Clear [Recent] vehicles list
8134T=Click this button to clear the [Recent] vehicles list.

8180=UI Font Size
8181=PAIRING BLUETOOTH DEVICE
8182=SEARCHING FOR BLUETOOTH DEVICES
8183=Bluetooth devices
8184=Device passkey
8185=Not found

8191=Indstillinger
8192=General
8193=Graf
8194=Interfaces
8197=Test
8197T=Testing connection with ELM/OBDKey interface.\rThe interface should be connected both to the computer and to the vehicle.\rAll responses should be OK.\rIf you get TIMEOUT error then you have probably set incorrect port speed.
8198=Annuler
8199=OK

8301=Detecting CANtieCAR interface ...
8302=Please make sure that the CANtieCAR interface is connected to the USB port and the driver is properly installed!
